1. J. Khan, M.H. Arsalan, Solar power technologies for sustainable electricity generation - a review, Renew. Sust. Energ. Rev. 55 (2016) 414–425, https://doi.org/10. 1016/j.rser.2015.10.135.
2. [2] D.J. Willis, C. Niezrecki, D. Kuchma, E. Hines, S.R. Arwade, R.J. Barthelmie, M. DiPaola, P.J. Drane, C.J. Hansen, M. Inalpolat, J.H. Mack, A.T. Myers, M. Rotea, Wind energy research: state-of-the-art and future research directions, Renew. Energy 125 (2018) 133–154, https://doi.org/10.1016/j.renene.2018.02.04

3G. Sundararajan, M. Roy, Solid particle erosion behavior of metallic materials atroom and elevated temperatures, Tribol. Int. 30 (5) (1997) 339–359.

4.

5. M.F. Morks, M.A. Shoeib, A. Ibrahim, Comparative study of nanostructured and

conventional WC-Co Coatings, in: ITSC2004, 2004: pp. 857–860

6. N. Abu-warda⁎ , A.J. López, M.D. López, M.V. Utrill High temperature corrosion and wear behavior of HVOF-sprayed coating of Al2O3-NiAl on AISI 304 stainless steel <https://doi.org/10.1016/j.surfcoat.2018.12.047>

## 7. Dipak K. Sarka [Pulverized Coal-Fired Boilers](https://www.sciencedirect.com/science/article/pii/B9780128015759000044) [Materials for Ultra-Supercritical and Advanced Ultra-Supercritical Power Plants](https://www.sciencedirect.com/book/9780081005521/materials-for-ultra-supercritical-and-advanced-ultra-supercritical-power-plants), 2017

8.Maria Oksa 1, Erja Turunen 1, Tomi Suhonen “Optimization and Characterization of High Velocity Oxy-fuelSprayed Coatings: Techniques, Materials, and Applications” *coatings* ISSN 2079-6412 *Coatings* 2011, *1*, 17-52www.mdpi.com/journal/coatings/

4.J. He, J.M. Schoenung, A review on nanostructured WC-Co coatings, Surf. Coatings

Technol. 157 (2002) 72–79

10A. H. Dent, S. Depalo, S. Sampath, Examina tion of the wear properties of HVOF

sprayed nanostructured and conventional WC-Co cermets with different binder

phase contents, J. Therm. Spray Technol. 11 (2002) 551–558.

11. Shigeaki Sugiyama, Daiki Kudo and Hitoshi Taimatsu, Preparation of WC-SiC Whisker Composites by Hot Pressingand Their Mechanical Properties, Materials Transactions, Vol. 49, No. 7 (2008)

12.Winarto Winarto, Nofrijon Sofyan and Didi Rooscote, Porosity and Wear Resistance of Flame Sprayed Tungsten Carbide Coatings, AIP Conference Proceedings 1855, 030012 (2017)

13 K. Murugan, A. Ragupathy, V. Balasubramanian, K. Sridhar, Optimizing HVOF

spray process parameters to attain minimum porosity and maximum hardness in

WC-10Co-4Cr coatings, Surf. Coatings Technol. 247 (2014) 90–102.

14 Q. Zhan, L. Yu, F. Ye, Q. Xue, H. Li, Quantitative evaluation of the decarburization

and microstructure evolution of WC-Co during plasma spraying, Surf. Coatings

Technol. 206 (2012) 4068–4074.

15.

16 Hsu SM, Shen MC. Ceramic wear maps. Wear 1996;200:154–7.

[17] Adachi K, Kato K, Chen N. Wear map of ceramics. Wear 1997;203–204:291–301.

18.Sandan Kumar Sharma, B. Venkata Manoj Kumaran, Young-Wook Kim, Effect of WC addition on sliding wear behaviour of SiC ceramics, Ceramics International 40 (2014) 6829–6839

  19*Serkan Islak1, Cihan Özorak1, Özkan Küçük1, Mehmet Akkaş2, Cihangir Tevfik Sezgin,* Microstructure and Hardness Properties of high velocity oxygen fuel (HVOF) Sprayed WCCo-SiC, *Kastamonu University Journal of Engineering and Sciences 1(1):1-7, 2015* Coatings

20. S. Tailor, R. M. Mohanty P. R. Soni ,Journal of Materials Science & Surface Engineering Vol. 1 (1), 2013, pp 15-0000

4

C. Fragassa, M. Ippoliti, *Failure Mode Effects and Criticality Analysis (FMECA) as a quality tool to plan improvements in Ultrasonic Mould Cleaning Systems*, International Journal for Quality Research, vol. 10, no. 4, pp. 847-870, 2016, doi: 10.18421/IJQR10.04-14

5.000 highB. Wang, S.W. Lee, Erosion-corrosion behaviour of HVOF NiAl-Al2O3 intermetallicceramic coating, Wear 239 (2000) 83–90, https://doi.org/10.1016/S0043- 1648(00)00309-4.

6. A. Di Gianfrancesco, in [Materials for Ultra-Supercritical and Advanced Ultra-Supercritical Power Plants](https://sci-hub.se/book/9780081005521/materials-for-ultra-supercritical-and-advanced-ultra-supercritical-power-plants), 2017